Tartalomjegyzék

[Kávézó terület 4](#_Toc161043684)

[Kávézó router 4](#_Toc161043685)

[EBEDLO VLAN 4](#_Toc161043686)

[BAR VLAN 4](#_Toc161043687)

[IRODA VLAN 4](#_Toc161043688)

[OSPF 4](#_Toc161043689)

[PPP 4](#_Toc161043690)

[GRE 4](#_Toc161043691)

[EBED\_S Switch 5](#_Toc161043692)

[VLAN 5](#_Toc161043693)

[Switchport mode 5](#_Toc161043694)

[VTP 5](#_Toc161043695)

[PORTVÉDELEM 5](#_Toc161043696)

[PORTÖSSZEFOGÁS 5](#_Toc161043697)

[Feszitő fa 5](#_Toc161043698)

[IRODA\_S switch 6](#_Toc161043699)

[Switchport mode 6](#_Toc161043700)

[VTP 6](#_Toc161043701)

[PORTVÉDELEM 6](#_Toc161043702)

[PORTÖSSZEFOGÁS 6](#_Toc161043703)

[Feszitő fa 6](#_Toc161043704)

[BAR\_S switch 7](#_Toc161043705)

[Switchport mode 7](#_Toc161043706)

[VTP 7](#_Toc161043707)

[PORTVÉDELEM 7](#_Toc161043708)

[PORTÖSSZEFOGÁS 7](#_Toc161043709)

[Feszitő fa 7](#_Toc161043710)

[NEW YORK HOTEL Terület 8](#_Toc161043711)

[RECEPCIO Switch 8](#_Toc161043712)

[VLANOK 8](#_Toc161043713)

[VTP 8](#_Toc161043714)

[Switchport mode 8](#_Toc161043715)

[SPANNING TREE 8](#_Toc161043716)

[PORTÖSSZEFOGÁS 8](#_Toc161043717)

[PORTVÉDELEM 9](#_Toc161043718)

[SECURITY Switch 9](#_Toc161043719)

[VTP 9](#_Toc161043720)

[Switchport mode 9](#_Toc161043721)

[SPANNING TREE 9](#_Toc161043722)

[IGAZGATOSAG Switch 9](#_Toc161043723)

[VTP 9](#_Toc161043724)

[Switchport mode 9](#_Toc161043725)

[SPANNING TREE 9](#_Toc161043726)

[PORTÖSSZEFOGÁS 10](#_Toc161043727)

[PORTVÉDELEM 10](#_Toc161043728)

[SZOBAK1 Switch 10](#_Toc161043729)

[VTP 10](#_Toc161043730)

[Switchport mode 10](#_Toc161043731)

[SPANNING TREE 11](#_Toc161043732)

[PORTÖSSZEFOGÁS 11](#_Toc161043733)

[PORTVÉDELEM 11](#_Toc161043734)

[SZOBAK2 Switch 11](#_Toc161043735)

[VTP 11](#_Toc161043736)

[Switchport mode 11](#_Toc161043737)

[SPANNING TREE 11](#_Toc161043738)

[PORTÖSSZEFOGÁS 12](#_Toc161043739)

[PORTVÉDELEM 12](#_Toc161043740)

[NewYorkHotel Router 12](#_Toc161043741)

[Recepció VLAN 12](#_Toc161043742)

[Security VLAN 12](#_Toc161043743)

[Hálószobák1 VLAN 12](#_Toc161043744)

[Igazgatóság VLAN 12](#_Toc161043745)

[Hálószobák2 VLAN 13](#_Toc161043746)

[VLAN 13](#_Toc161043747)

[OSPF 13](#_Toc161043748)

[PPP 13](#_Toc161043749)

[HSRP 13](#_Toc161043750)

[DHCP 14](#_Toc161043751)

[Backup router 14](#_Toc161043752)

[Static route 14](#_Toc161043753)

[OSPF 14](#_Toc161043754)

[Recepció VLAN 15](#_Toc161043755)

[Security VLAN 15](#_Toc161043756)

[Hálószobák1 VLAN 15](#_Toc161043757)

[Igazgatóság VLAN 15](#_Toc161043758)

[Hálószobák2 VLAN 15](#_Toc161043759)

[VLAN 15](#_Toc161043760)

[HSRP 16](#_Toc161043761)

[DHCP 16](#_Toc161043762)

[PAT 17](#_Toc161043763)

[Üzemeltetők terület 18](#_Toc161043764)

[Üzemeltetők router 18](#_Toc161043765)

[Static route 18](#_Toc161043766)

[OSPF 18](#_Toc161043767)

[PPP 18](#_Toc161043768)

[GRE 18](#_Toc161043769)

[ACL 18](#_Toc161043770)

[PAT 18](#_Toc161043771)

[Laguna Motel Terület 20](#_Toc161043772)

[Laguna Motel router 20](#_Toc161043773)

[OSPF 20](#_Toc161043774)

[PPP 20](#_Toc161043775)

[Távmunkás Terület 21](#_Toc161043776)

[Home router 21](#_Toc161043777)

[Static route 21](#_Toc161043778)

[ISP Terület 22](#_Toc161043779)

[ISP router 22](#_Toc161043780)

[Config 22](#_Toc161043781)

[IP Címzés 22](#_Toc161043782)

[Static route 22](#_Toc161043783)

# Kávézó terület

## Kávézó router

### EBEDLO VLAN

int gig0/0.10

encap dot1q 10

ip add 192.168.31.1 255.255.255.128

### BAR VLAN

int gig0/0.20

encap dot1q 20

ip add 192.168.31.129 255.255.255.192

### IRODA VLAN

int gig0/0.30

encap dot1q 30

ip add 192.168.31.193 255.255.255.248

### OSPF

router ospf 1

router-id 3.3.3.3

passive-interface gig0/0

network 192.168.31.0 0.0.0.127 area 0

network 192.168.31.128 0.0.0.63 area 0

network 192.168.31.192 0.0.0.7 area 0

network 100.100.100.12 0.0.0.3 area 0

network 100.100.100.20 0.0.0.3 area 0

### PPP

Még üres :’)

### GRE

int t1

ip address 200.200.200.2 255.255.255.252

tunnel source se0/0/1

tunnel destination 100.100.100.18

## EBED\_S Switch

### VLAN

vlan 10

name EBEDLO

vlan 20

name BAR

vlan 30

name IRODA

### Switchport mode

int gig0/1

sw mo trunk

int range fa0/1-6

sw mo trunk

### VTP

vtp mode server

vtp domain kavezo

vtp password kave123

vtp version 2

### PORTVÉDELEM

int range f0/5-24

sh

int range gig0/1-2, f0/1-4

switchport port-security mac-address sticky

switchport port-security violation restrict

switchport port-security maximum 1

### PORTÖSSZEFOGÁS

int range f0/1-2

channel-group 1 mode desirable

int range f0/3-4

channel-group 2 mode desirable

### Feszitő fa

spanning-tree mode rapid-pvst

spanning-tree vlan 10,20,30 root primary

int gig0/2

spanning-tree portfast

spanning-tree bpduguard enable

## IRODA\_S switch

### Switchport mode

int range fa0/1-6

sw mo trunk

int range fa0/3-4, fa0/24

sw mode acc

sw acc vlan 30

### VTP

vtp mode client

vtp domain kavezo

vtp password kave123

### PORTVÉDELEM

int range f0/7-23

sh

int range f0/1-6, f0/24

switchport port-security mac-address sticky

switchport port-security violation restrict

switchport port-security maximum 1

### PORTÖSSZEFOGÁS

int range f0/1-2

channel-group 1 mode desirable

int range f0/5-6

channel-group 3 mode desirable

### Feszitő fa

spanning-tree mode rapid-pvst

spanning-tree vlan 10,20,30 root secondary

int range f0/3-4, f0/24

spanning-tree portfast

spanning-tree bpduguard enable

## BAR\_S switch

### Switchport mode

int range fa0/1-6

sw mo trunk

int range fa0/2

sw mode acc

sw acc vlan 20

### VTP

vtp mode client

vtp domain kavezo

vtp password kave123

### PORTVÉDELEM

int range f0/1, f0/7-24, gig0/1

sh

int range f0/2-6, gig0/2

switchport port-security mac-address sticky

switchport port-security violation restrict

switchport port-security maximum 1

### PORTÖSSZEFOGÁS

int range f0/3-4

channel-group 2 mode desirable

int range f0/5-6

channel-group 3 mode desirable

### Feszitő fa

spanning-tree mode rapid-pvst

int range gig0/2, f0/2

spanning-tree portfast

spanning-tree bpduguard enable

# NEW YORK HOTEL Terület

## RECEPCIO Switch

### VLANOK

vlan 11

name RECEPCIO

vlan 12

name SECURITY

vlan 21

name HALO1

vlan 22

name IGAZGATOSAG

vlan 31

name HALO2

### VTP

vtp domain NYHOTEL

vtp version 2

vtp password NYHOTEL

### Switchport mode

int range fa0/21-24

switchport mode access

switchport access vlan 11

int range gig0/1, fa0/1-6

switchport mode trunk

### SPANNING TREE

spanning-tree mode rapid-pvst

spanning-tree vlan 11,12,21,22,31 root primary

int range fa0/21-24

spanning-tree portfast

spanning-tree bpduguard enable

### PORTÖSSZEFOGÁS

int range fa0/1-2

channel-group 1 mode desirable

int port-channel 1

switchport mode trunk

int range fa0/5-6

channel-group 2 mode desirable

int port-channel 2

switchport mode trunk

int range fa0/3-4

channel-group 3 mode desirable

int port-channel 3

switchport mode trunk

### PORTVÉDELEM

int range f0/7-20, gig0/2

sh

int range gig0/1, f0/1-6, f0/21-24

switchport port-security mac-address sticky

switchport port-security violation restrict

switchport port-security maximum 1

## SECURITY Switch

### VTP

vtp mode client

vtp domain NYHOTEL

vtp password NYHOTEL

### Switchport mode

int range fa0/22-24

switchport mode access

switchport access vlan 12

### SPANNING TREE

spanning-tree mode rapid-pvst

spanning-tree vlan 11,12,21,22,31 root secondary

int range fa0/22-24

spanning-tree bpduguard enable

spanning-tree portfast

## IGAZGATOSAG Switch

### VTP

vtp mode client

vtp domain NYHOTEL

vtp password NYHOTEL

### Switchport mode

int range fa0/22-24

switchport mode access

switchport access vlan 22

### SPANNING TREE

spanning-tree mode rapid-pvst

int range fa0/23-24

spanning-tree portfast

spanning-tree bpduguard enable

### PORTÖSSZEFOGÁS

int range fa0/1-2

channel-group 6 mode desirable

int port-channel 6

switchport mode trunk

int range fa0/3-4

channel-group 4 mode desirable

int port-channel 4

switchport mode trunk

int range fa0/5-6

channel-group 2 mode desirable

int port-channel 2

switchport mode trunk

### PORTVÉDELEM

int range f0/7-21, gig0/1-2

sh

int range f0/1-6, f0/22-24 ?

switchport port-security mac-address sticky

switchport port-security violation restrict

switchport port-security maximum 1

## SZOBAK1 Switch

### VTP

vtp mode client

vtp domain NYHOTEL

vtp password NYHOTEL

### Switchport mode

int fa0/24

switchport mode access

switchport access vlan 21

### SPANNING TREE

spanning-tree mode rapid-pvst

int fa0/24

spanning-tree bpduguard enable

### PORTÖSSZEFOGÁS

int range fa0/1-2

channel-group 5 mode desirable

int port-channel 5

switchport mode trunk

int range fa0/3-4

channel-group 3 mode desirable

int port-channel 3

switchport mode trunk

### PORTVÉDELEM

int range f0/5-23, gig0/1-2

sh

int range f0/1-4, f0/24 ?

switchport port-security mac-address sticky

switchport port-security violation restrict

switchport port-security maximum 1

## SZOBAK2 Switch

### VTP

vtp mode client

vtp domain NYHOTEL

vtp password NYHOTEL

### Switchport mode

int fa0/24

switchport mode access

switchport access vlan 31

### SPANNING TREE

spanning-tree mode rapid-pvst

int fa0/24

spanning-tree bpduguard enable

### PORTÖSSZEFOGÁS

int range fa0/1-2

channel-group 5 mode desirable

int port-channel 5

switchport mode trunk

int range fa0/3-4

channel-group 6 mode desirable

int port-channel 6

switchport mode trunk

### PORTVÉDELEM

int range f0/5-23, gig0/1-2

sh

int range f0/1-4, f0/24 ?

switchport port-security mac-address sticky

switchport port-security violation restrict

switchport port-security maximum 1

## NewYorkHotel Router

### Recepció VLAN

int gig0/0.11

encapsulation dot1q 11

ip add 172.16.0.81 255.255.255.248

### Security VLAN

int gig0/0.12

encapsulation dot1q 12

ip add 172.16.0.89 255.255.255.248

### Hálószobák1 VLAN

int gig0/0.21

encapsulation dot1q 21

ip add 172.16.0.1 255.255.255.224

### Igazgatóság VLAN

int gig0/0.22

encapsulation dot1q 22

ip add 172.16.0.65 255.255.255.248

### Hálószobák2 VLAN

int gig0/0.31

encapsulation dot1q 31

ip add 172.16.0.33 255.255.255.224

### VLAN

int gig0/0

no sh

### OSPF

router ospf 1

router-id 2.2.2.2

passive-interface gig0/0

passive-interface gig0/0.11

passive-interface gig0/0.12

passive-interface gig0/0.21

passive-interface gig0/0.22

passive-interface gig0/0.31

network 172.16.0.0 0.0.0.31 area 0

network 172.16.0.32 0.0.0.31 area 0

network 172.16.0.64 0.0.0.7 area 0

network 172.16.0.80 0.0.0.7 area 0

network 172.16.0.88 0.0.0.7 area 0

network 100.100.100.28 0.0.0.3 area 0

network 100.100.100.20 0.0.0.3 area 0

### PPP

Még üres

### HSRP

int g0/0.11

standby ver 2

standby 11 ip 172.16.0.86

standby 11 priority 150

standby 11 preempt

int g0/0.12

standby ver 2

standby 12 ip 172.16.0.94

standby 12 priority 150

standby 12 preempt

int g0/0.21

standby ver 2

standby 21 ip 172.16.0.30

standby 21 priority 150

standby 21 preempt

int g0/0.22

standby ver 2

standby 22 ip 172.16.0.78

standby 22 priority 150

standby 22 preempt

int g0/0.31

standby ver 2

standby 31 ip 172.16.0.62

standby 31 priority 150

standby 31 preempt

### DHCP

ip dhcp pool VLAN21

network 172.16.0.0 255.255.255.224

default-router 172.16.0.30

ip dhcp pool VLAN31

network 172.16.0.32 255.255.255.224

default-router 172.16.0.62

ip dhcp excluded-address 172.16.0.81

ip dhcp excluded-address 172.16.0.89

ip dhcp excluded-address 172.16.0.1

ip dhcp excluded-address 172.16.0.2

ip dhcp excluded-address 172.16.0.82

ip dhcp excluded-address 172.16.0.90

ip dhcp excluded-address 172.16.0.33

ip dhcp excluded-address 172.16.0.34

ip dhcp excluded-address 172.16.0.65

ip dhcp excluded-address 172.16.0.66

ip dhcp excluded-address 172.16.0.86

ip dhcp excluded-address 172.16.0.94

ip dhcp excluded-address 172.16.0.30

ip dhcp excluded-address 172.16.0.62

ip dhcp excluded-address 172.16.0.78

## Backup router

### Static route

ip route 0.0.0.0 0.0.0.0 gig0/2/0

### OSPF

router ospf 1

router-id 5.5.5.5

network 100.100.100.36 0.0.0.3 area 0

network 100.100.100.32 0.0.0.3 area 0

network 100.100.100.40 0.0.0.3 area 0

network 172.16.0.0 0.0.0.31 area 0

network 172.16.0.32 0.0.0.31 area 0

network 172.16.0.64 0.0.0.7 area 0

network 172.16.0.80 0.0.0.7 area 0

network 172.16.0.88 0.0.0.7 area 0

network 100.100.100.28 0.0.0.3 area 0

network 100.100.100.20 0.0.0.3 area 0

passive-interface gig0/0

passive-interface gig0/0.11

passive-interface gig0/0.12

passive-interface gig0/0.21

passive-interface gig0/0.22

passive-interface gig0/0.31

passive-interface gig0/2/0

default-information originate

### Recepció VLAN

int gig0/0.11

encapsulation dot1q 11

ip add 172.16.0.82 255.255.255.248

### Security VLAN

int gig0/0.12

encapsulation dot1q 12

ip add 172.16.0.90 255.255.255.248

### Hálószobák1 VLAN

int gig0/0.21

encapsulation dot1q 21

ip add 172.16.0.2 255.255.255.224

### Igazgatóság VLAN

int gig0/0.22

encapsulation dot1q 22

ip add 172.16.0.66 255.255.255.248

### Hálószobák2 VLAN

int gig0/0.31

encapsulation dot1q 31

ip add 172.16.0.34 255.255.255.224

### VLAN

int gig0/0

no sh

### HSRP

int g0/0.11

standby ver 2

standby 11 ip 172.16.0.86

int g0/0.12

standby ver 2

standby 12 ip 172.16.0.94

int g0/0.21

standby ver 2

standby 21 ip 172.16.0.30

int g0/0.22

standby ver 2

standby 22 ip 172.16.0.78

int g0/0.31

standby ver 2

standby 31 ip 172.16.0.62

### DHCP

ip dhcp pool VLAN21

network 172.16.0.0 255.255.255.224

default-router 172.16.0.30

ip dhcp pool VLAN31

network 172.16.0.32 255.255.255.224

default-router 172.16.0.62

ip dhcp excluded-address 172.16.0.81

ip dhcp excluded-address 172.16.0.89

ip dhcp excluded-address 172.16.0.1

ip dhcp excluded-address 172.16.0.2

ip dhcp excluded-address 172.16.0.82

ip dhcp excluded-address 172.16.0.90

ip dhcp excluded-address 172.16.0.33

ip dhcp excluded-address 172.16.0.34

ip dhcp excluded-address 172.16.0.65

ip dhcp excluded-address 172.16.0.66

ip dhcp excluded-address 172.16.0.86

ip dhcp excluded-address 172.16.0.94

ip dhcp excluded-address 172.16.0.30

ip dhcp excluded-address 172.16.0.62

ip dhcp excluded-address 172.16.0.78

### PAT

int gig0/2/0

ip nat outside

int gig0/0

ip nat inside

int se0/1/0

ip nat inside

int se0/0/0

ip nat inside

ip access-list standard 60

permit 35.125.55.0 0.0.0.127

permit 192.168.54.0 0.0.0.31

permit 192.168.54.32 0.0.0.7

permit 192.168.31.0 0.0.0.127

permit 192.168.31.248 0.0.0.7

permit 192.168.31.128 0.0.0.63

permit 172.16.0.80 0.0.0.7

permit 172.16.0.88 0.0.0.7

permit 172.16.0.0 0.0.0.31

permit 172.16.0.64 0.0.0.15

permit 172.16.0.32 0.0.0.31

ip nat pool PATPOOL2 51.51.51.51 51.51.51.51 netmask 255.255.255.0

ip nat inside source list 60 pool PATPOOL2 overload

# Üzemeltetők terület

## Üzemeltetők router

### Static route

ip route 0.0.0.0 0.0.0.0 gig0/0/0

### OSPF

router ospf 1

router-id 1.1.1.1

passive-interface gig0/0

passive-interface gig0/0/0

network 35.125.55.0 0.0.0.127 area 0

network 100.100.100.28 0.0.0.3 area 0

network 100.100.100.16 0.0.0.3 area 0

network 100.100.100.20 0.0.0.3 area 0

default-information originate

### PPP

int se0/1/0

encap ppp

ppp authentication chap

exit

username Laguna secret cisco

### GRE

int t1

ip address 200.200.200.1 255.255.255.252

tunnel source se0/1/0

tunnel destination 100.100.100.22

### ACL

Üzemeltetők

ip access-list extended noping

deny icmp any host 35.125.55.126 echo

deny icmp any host 35.125.55.125 echo

deny icmp any host 35.125.55.124 echo

deny icmp any host 35.125.55.123 echo

int g0/0

ip access-group noping out

### PAT

int gig0/0

ip nat inside

int se0/1/0

ip nat inside

int se0/1/1

ip nat inside

int se0/2/0

ip nat inside

int gig0/0/0

ip nat outside

ip access-list standard 60

permit 35.125.55.0 0.0.0.127

permit 192.168.54.0 0.0.0.31

permit 192.168.54.32 0.0.0.7

permit 192.168.31.0 0.0.0.127

permit 192.168.31.248 0.0.0.7

permit 192.168.31.128 0.0.0.63

permit 172.16.0.80 0.0.0.7

permit 172.16.0.88 0.0.0.7

permit 172.16.0.0 0.0.0.31

permit 172.16.0.64 0.0.0.15

permit 172.16.0.32 0.0.0.31

ip nat pool PATPOOL1 50.50.50.50 50.50.50.50 netmask 255.255.255.0

ip nat inside source list 60 pool PATPOOL1 overload

# Laguna Motel Terület

## Laguna Motel router

### OSPF

router ospf 1

router-id 4.4.4.4

passive-interface gig0/0

passive-interface gig0/1

network 192.168.54.40 0.0.0.3 area 0

network 192.168.54.32 0.0.0.7 area 0

network 100.100.100.16 0.0.0.3 area 0

network 100.100.100.12 0.0.0.3 area 0

### PPP

int se0/0/0

encap ppp

ppp authentication chap

exit

username Uzemeltetok secret cisco

# Távmunkás Terület

## Home router

### Static route

ip route 0.0.0.0 0.0.0.0 gig0/0/0

# ISP Terület

## ISP router

### Config

Hostname

hostname ISP\_R

### IP Címzés

Interface GIG0/0

ip address 100.100.100.1 255.255.255.248

Interface GIG0/0/0

ip address 100.100.100.25 255.255.255.252

Interface GIG0/1/0

ip address 100.100.100.9 255.255.255.252

### Static route

ip route 0.0.0.0 0.0.0.0 gig0/0/0

ip route 100.100.100.8 255.255.255.252 100.100.100.10